A Big Earth Data Platform for Three Poles

**HiWATER: Dataset of intensive runoff observations of No.3 in the midstream of the Heihe River Basin of the MUlti-Scale Observation EXperiment on Evapotranspiration over heterogeneous land surfaces 2012 (MUSOEXE-12)**

1、Description

The No. 3 hydrological section is located at Railway Heihe River Bridge (39°02′33.08″ N, 100° 25′49.42″ E, 1443 m a.s.l.) in the middle reaches of the Heihe River Basin, Zhangye, Gansu Province. The dataset contains observations from the No.3 hydrological section from 14 June, 2012, to 24 November, 2012. The width of this section is 50 meters. The water level was measured using SR50 ultrasonic range and the discharge was measured using cross-section reconnaissance by the StreamPro ADCP. The dataset includes the following sections: Water level (recorded every 30 minutes) and Discharge. The data processing and quality control steps were as follows: 1) The water level data which collected from the hydrological station were averaged over intervals of 10 min for a total of 144 records per day. The missing data were denoted by -6999. 2) Data out the normal range records were rejected. 3) Unphysical data were rejected.
For more information, please refer to Liu et al. (2016) (for multi-scale observation experiment or sites information), He et al. (2016) (for data processing) in the Citation section.

2、Keywords

Theme：Surface Water,Hydrology section,Discharge/Flow,Runoff
Discipline：Terrestrial Surface
Places：Heihe River Basin, the artificial oasis experimental area in the middle reaches, No.3 Railway Bridge
Time：2012, 2012-06-14 to 2012-11-24

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：0.21MB

4.Data format：EXCEL

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：39.041944 | - |
| west：100.432778 | - | east：100.433056 |
| - | south：39.04222 | - |

5、Time frame:2012-06-24 08:31:00+00:00--2012-12-04 08:31:00+00:00

6、Reference method

References to data:

LIU Shaomin, JIANG Heng. HiWATER: Dataset of intensive runoff observations of No.3 in the midstream of the Heihe River Basin of the MUlti-Scale Observation EXperiment on Evapotranspiration over heterogeneous land surfaces 2012 (MUSOEXE-12). A Big Earth Data Platform for Three Poles, doi:10.3972/hiwater.111.2013.db2016

References to articles:

He XB, et al. Comparison of a tipping-buchet and electronic weighting precipitation gauge for rainfall. Manuscript in preparation.

Li, X., Cheng, G.D., Liu, S.M., Xiao, Q., Ma, M.G., Jin, R., Che, T., Liu, Q.H., Wang, W.Z., Qi, Y., Wen, J.G., Li, H.Y., Zhu, G.F., Guo, J.W., Ran, Y.H., Wang, S.G., Zhu, Z.L., Zhou, J., Hu, X.L., & Xu, Z.W. (2013). Heihe watershed allied telemetry experimental research (hiwater): scientific objectives and experimental design. Bulletin of the American Meteorological Society, 94(8), 1145-1160. doi:10.1175/BAMS-D-12-00154.1.

7、Supporting project information

National Natural Science Foundation of China

8、Data resource provider

name: JIANG Heng
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences
email:

name: LIU Shaomin
unit: Beijing Normal University
email: smliu@bnu.edu.cn