A Big Earth Data Platform for Three Poles

**HiWATER: Airborne CCD image data in the midstream of Heihe River Basin（2012.08.02）**

1、Description

On 2 August 2012, Wide-angle Infrared Dual-mode line/area Array Scanner (WIDAS) carried by the Harbin Y-12 aircraft was used in a visible near Infrared thermal Dual-mode airborne remote sensing experiment, which is located in the artificial oasis eco-hydrology experimental area (30×30 km). WIDAS includes a CCD camera with a spatial resolution of 0.26 m, a visible near Infrared multispectral camera with five bands scanner (an maximum observation angle 48° and spatial resolution 1.3 m), and a thermal image camera with a spatial resolution of 6.3 m.
The CCD camera data are recorded in DN values processed by mosaic and orthorectification.

2、Keywords

Theme：Remote Sensing Technology,Wide-angle infrared dual-mode line/Area array scanner,CCD
Discipline：Remote Sensing Technology
Places：Heihe River Basin, the artificial oasis experimental area in the middle reaches
Time：2012, 2012-08-02

3、Data details

1.Scale：None

2.Projection：WGS84 UTM

3.Filesize：46899.2MB

4.Data format：tif

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：39.0 | - |
| west：100.3 | - | east：100.46 |
| - | south：38.7 | - |

5、Time frame:2018-11-25 10:51:15+00:00--2018-11-25 10:51:15+00:00

6、Reference method

References to data:

Wen Jianguang. HiWATER: Airborne CCD image data in the midstream of Heihe River Basin（2012.08.02）. A Big Earth Data Platform for Three Poles, doi:10.3972/hiwater.163.2014.db2018

References to articles:

Li, X., Liu, S.M., Xiao, Q., Ma, M.G., Jin, R., Che, T., Wang, W.Z., Hu, X.L., Xu, Z.W., Wen, J.G., Wang, L.X. (2017). A multiscale dataset for understanding complex eco-hydrological processes in a heterogeneous oasis system. Scientific Data, 4, 170083. doi:10.1038/sdata.2017.83.

7、Supporting project information

Heihe Watershed Allied Telemetry Experimental Research (HiWATER)

8、Data resource provider

name: Wen Jianguang
unit:
email: wenjg@irsa.ac.cn