A Big Earth Data Platform for Three Poles

**The Landsat MSS image Datasets over Heihe River Basin (1972-1978)**

1、Description

On July 23, 1972, the United States launched the world's first resource satellite "Landsat 1" , and Landsat 2 and Landsat 3 were launched in the following 10 years. These three satellites were the first generation of resource satellites. They were equipped withreturn-beam vidicon cameras and multi-spectral scanners (MSS) with 3 and 4 spectral segments respectively, a resolution of 79m and a width of 185Km.
There are 28 scenes of MSS data in Heihe River Basin currently which were obtained on the following dates: 1972-10-14, 1972-10-30, 1973-01-10, 1973-01-31, 1973-02-16, 1973-06-04, 1973. -10-07, 1973-10-28 (2 scenes), 1973-12-22, 1974-01-05, 1975-10-07, 1975-10-09, 1976-07-04, 1976-10-18 , 1976-11-07, 1976-11-27, 1976-12-30, 1977-01-19, 1977-02-07, 1977-04-20, 1977-05-06 (2 scenes), 1977-05 -08, 1977-06-10, 1977-06-29, 1977-07-18, 1978-10-09.
Ortho rectification was performed on the images.

2、Keywords

Theme：Remote Sensing Technology,Visible remote sensing
Discipline：Remote Sensing Technology
Places：Heihe River Basin
Time：1972 to 1978

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：1676.93MB

4.Data format：栅格

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：43.3 | - |
| west：96.1 | - | east：104.2 |
| - | south：37.7 | - |

5、Time frame:1972-07-09 12:00:00+00:00--1978-12-23 15:13:00+00:00

6、Reference method

References to data:

LP DAAC User Services. The Landsat MSS image Datasets over Heihe River Basin (1972-1978). A Big Earth Data Platform for Three Poles, 2013

References to articles:

7、Supporting project information

8、Data resource provider

name: LP DAAC User Services
unit: USGS Earth Resources Observation and Science (EROS) Center
email: lpdaac@eos.nasa.gov